SDK for: RUD2v2, RUD3v1, RUD3v2, RUD4v1 v1.0.6
Copyright Roger Sp.zoo.Sp.k.
=======================================================================

SDK for RUD2v2, RUD3v1, RUD3v2, RUD4v1 includes libraries, documentation and C# .NET examples.

RogerReaderExample allows to read EM 125kHz proximity cards with RUD2v2 or RUD4v1  
reader and to read/write Mifare cards with RUD3v1, RUD3v2 or RUD4v1 reader 
according to read/write rules configured with RogerVDM software (available at www.roger.pl).

RUD4Tester is strictly dedicated to RUD4v1 reader and in addition to reading of EM 125kHz 
and Mifare cards it enables to handle LED indicators, buzzer and internal relay.

RUDs documentation explains EPSO2 command structure used for communication with USB-HID  
class RUD devices.


SDK for RUD2v2, RUD3v1, RUD3v2, RUD4v1 v1.0.6            26.05.2021
-------------------------------------------------------------------
Includes folowing components,

Libraries:
RogerRUD3.dll v 1.1.0.2
RogerUsbHid.dll v 1.0.2.4
RogerMifare v 1.0.0.0

C# .NET example:
RogerReaderExample v1.0.8.006
RUD4Tester v1.0.2.002

Documentation:
RUDs v1.0